Stroom meting

Ina169

High side measurement

Analog output

Vcc: 2.7V – 60V

Ina219

I2C

Integrated adc

Programable addresses

Vcc: -0.3V to 26V

Acs712

Vcc: 4.5V – 5.5V

Measures current with zero amps at 2.5V

Werking getest maar niet ideaal